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Magnus Plus RZ2KR#4S – 2KV
On-line UPS (Rack & Tower)
· True online double-conversion UPS.
· Zero transfer time with pure sinewave output.
· High output power factor for efficient load support.
· Suitable for IT, hospital, commercial, and critical applications. 

Overview
The Magnus Plus Series: is an online UPS range designed to deliver continuous and reliable power protection for IT, commercial, and critical applications.
Using true double-conversion technology, it delivers pure sinewave output, stable voltage, and zero transfer time to protect sensitive equipment from all power disturbances.

Rated Output: 2000VA / 1800W
Battery: 4 × 12V 9Ah
Transfer Time: 0 ms
Output Wave: Pure Sinewave

Features:
· Double-conversion online UPS topology.
· Pure sinewave output under all operating conditions.
· High output power factor (up to 0.9).
· Wide input voltage and frequency tolerance.
· Advanced digital control and monitoring.
· Comprehensive protection functions (overload, short-circuit, battery protection).
· Cold start capability.
